**PDA :**

Design PDA for the input a^nb^n

